{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Item Number","Title","Document Number","Quantity"]
[1,"FH Die Plate","346 x 396 x 46",1]
[2,"MH Die Plate","346 x 396 x 46",1]
[3,"Support Plate","346 x 396 x 46",1]
[4,"Ejector Plate Top","396 x 252 x 16",1]
[5,"Ejector Plate Bottom","396 x 252 x 26",1]
[6,"Riser","396 x 46 x 86",2]
[7,"MH Clamping Plate","346 x 396 x 26",1]
[8,"FH Clamping Plate","346 x 396 x 26",1]
[9,"Sprue Bush","Dia 18 - 53",1]
[10,"Locating Ring","LR-125",1]
[11,"Locating Bush","FBN24-46",4]
[12,"Locating Pin","FSN24-46-46",4]
[]
[]
[13,"Angle Pin","D 12-65",8]
[14,"Ejector Pin","D 5 x 250",8]
[15,"Ejector Pin","D 6 x 200",1]
[16,"Ejector Pin","D 6.5 x 100",4]
[17,"Sleeve Ejector Pin","OD 8 - ID 5 x 150",8]
[]
[null,"Took Steel Plates"]
[18,"MH Core","231 x 200 x 64",1]
[19,"Slide A","180 x 69 x 34",2]
[20,"Slide B","190 x 64 x 34",2]
[21,"Rail B","50 x 15 x 7",4]
[22,"Rail A","55 x 15 x 7",4]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}